


Hardware detail:







Circuit:

1 - +12V (Power Supply)

2- GND (Circuit)

3 - VRS1+

4 - VRS1-

5 - KEY

6 – TEMP

7 - HIGH\_VOLTAGE (Ignition Coil)

8 - GROUND (Ignition Coil)

I need to decide If I populate the circuit or if I do not populate…

VRS2+

VRS2-

CAN\_HIGH

CAN\_LOW

INJECTOR

TPS\_VCC

TPS\_SIGNAL

TPS\_GROUND

TEMP\_SENSOR